#!dimctrl --exec

# ==========================================================================
# check feedback state before switching BIAS ON and ramping up to nominal Voltage
# ==========================================================================

> checking feedback state
.s FEEDBACK 12      # Current Control
> ... Current/Temp control active and voltage output enabled
> switching on bias ...

BIAS_CONTROL/SET_GLOBAL_DAC 1
.s BIAS_CONTROL 9   # Voltage ON
> ...set 1 DAC
.s BIAS_CONTROL 5   # Ramping
> ...ramping
.s BIAS_CONTROL 9   # Voltage ON
> ...bias ON

# here one should wait 30..45sec according to TB
> bias is on, and feedback-program is working, but we wait 45sec for the current readings...
.w 45000
> ... done
