#!dimctrl --exec

# ==========================================================================
# Script for taking data when you are tracking wobble position 1

# take a DRS CaLibration and physics Data afterwards
# ==========================================================================

# Move Telescope to Wobble Position 1
>
> -----------
> data taking script for Wobble 1 starting up...
> -----------
>
> Operator: make sure that telescope is tracking wobble position 1 of source
>

# Take a DRS-Calibration before beginning to take physics Data
.x ScriptsForDimCtrl/ServiceScripts/TakeDrsCalibration.dim

> Operator: make sure that telescope is tracking correct wobble position of source
>
> Operator: Measure Sky Brightness

# check feedback state before switching BIAS ON and ramping up to nominal Voltage
.x ScriptsForDimCtrl/ServiceScripts/PrepareBiasForDataTaking.dim

# taking a Data Set (1x Pedestal 1000 Bias On, 1x LPext 1000, 4x5min DataRun)
.x ScriptsForDimCtrl/ServiceScripts/TakeData.dim

> ----------------------------------------------------
> This is the end of data taking of Wobble 1
> ----------------------------------------------------
