#!dimctrl --exec

# ==========================================================================
# Checking the system statuses if they are ready for data taking
# ==========================================================================

>
> Checking the system statuses
> ...checking DRIVE
# 7 = Tracking
.s DRIVE_CONTROL 7

> ...checking FEEDBACK
# 12 = CurrentControl
.s FEEDBACK 12

> ...checking BIAS
# 9 = VoltageOn
.s BIAS_CONTROL 9

> ...checking FAD
# 4 = Connected
.s FAD_CONTROL 4
> ...system statuses OK
