FACT
|<h4>Trigger rate</h4>
If the dim network is online and the trigger master (ftmctrl) in in state
TriggerOn, the current camera trigger rate is displayed. If the
bias voltage is swicthed on (biasctrl in state VoltageOn), also the
median patch threshold is displayed in ()-parenthesis.

<ul class='help'>
<li>Trigger rate between 15Hz and 100Hz</li>
<li>Trigger rate below 15Hz</li>
<li>Trigger rate above 100Hz</li>
</ul>
|
