Camera
|image=fact-camera.png|
|
The camera display is available in different types. It can display 40
(board) values, 160 (patch) values, 320 (bias channel) values or
1440 pixels. Depending on the type of input data several pixels mights
consequently be displayed in the same color.
|
|<h4>min / med /max</h4>
The minimum, median and maximum value of all values displayed in the camera.
|
|<h4>Scale</h4>
The color scale of the displayed data.
|
