#!dimctrl --exec

# This sript takes a DRS Calibration for data of ROI=1024
# Making sure bias is off
.! echo `date -u` "First DRS Calibration Script starting up..." >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log
.! echo `date -u` "-------------------------------------------" >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log
FEEDBACK/ENABLE_OUTPUT 1
BIAS_CONTROL/SET_ZERO_VOLTAGE
.s BIAS_CONTROL 7
FAD_CONTROL/START_DRS_CALIBRATION
.! echo `date -u` "bias voltage is switched off" >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log

.! echo `date -u` "taking DRS:Pedestal 1000 ..." >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log
MCP/START -1 1000 drs-pedestal
.s FAD_CONTROL 8
.s FAD_CONTROL 4
.! echo `date -u` "... done" >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log

.! echo `date -u` "taking DRS:Gain 1000 ..." >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log
MCP/START -1 1000 drs-gain
.s FAD_CONTROL 8
.s FAD_CONTROL 4
.! echo `date -u` "... done" >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log

.! echo `date -u` "taking DRS:Pedestal 1000 ..." >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log
MCP/START -1 1000 drs-pedestal
.s FAD_CONTROL 8
.s FAD_CONTROL 4
.! echo `date -u` "... done" >> ~/FACT++/ScriptsForDimCtrl/DataTaking.log

