#!dimctrl --exec

> connecting to requested crate...

# connect to crate 0
: 0
.w 3800
FAD_CONTROL/CONNECT 0
.w 3800
FAD_CONTROL/CONNECT 1
.w 3800
FAD_CONTROL/CONNECT 2
.w 3800
FAD_CONTROL/CONNECT 3
.w 3800
FAD_CONTROL/CONNECT 4
.w 3800
FAD_CONTROL/CONNECT 5
.w 3800
FAD_CONTROL/CONNECT 6
.w 3800
FAD_CONTROL/CONNECT 7
.w 3800
FAD_CONTROL/CONNECT 8
.w 3800
FAD_CONTROL/CONNECT 9
.j 255

# connect to crate 1
: 1
FAD_CONTROL/CONNECT 10
.w 3800
FAD_CONTROL/CONNECT 11
.w 3800
FAD_CONTROL/CONNECT 12
.w 3800
FAD_CONTROL/CONNECT 13
.w 3800
FAD_CONTROL/CONNECT 14
.w 3800
FAD_CONTROL/CONNECT 15
.w 3800
FAD_CONTROL/CONNECT 16
.w 3800
FAD_CONTROL/CONNECT 17
.w 3800
FAD_CONTROL/CONNECT 18
.w 3800
FAD_CONTROL/CONNECT 19
.j 255

# connect to crate 2
: 2
FAD_CONTROL/CONNECT 20
.w 3800
FAD_CONTROL/CONNECT 21
.w 3800
FAD_CONTROL/CONNECT 22
.w 3800
FAD_CONTROL/CONNECT 23
.w 3800
FAD_CONTROL/CONNECT 24
.w 3800
FAD_CONTROL/CONNECT 25
.w 3800
FAD_CONTROL/CONNECT 26
.w 3800
FAD_CONTROL/CONNECT 27
.w 3800
FAD_CONTROL/CONNECT 28
.w 3800
FAD_CONTROL/CONNECT 29

.j 255

# connect to crate 3
: 3
FAD_CONTROL/CONNECT 30
.w 3800
FAD_CONTROL/CONNECT 31
.w 3800
FAD_CONTROL/CONNECT 32
.w 3800
FAD_CONTROL/CONNECT 33
.w 3800
FAD_CONTROL/CONNECT 34
.w 3800
FAD_CONTROL/CONNECT 35
.w 3800
FAD_CONTROL/CONNECT 36
.w 3800
FAD_CONTROL/CONNECT 37
.w 3800
FAD_CONTROL/CONNECT 38
.w 3800
FAD_CONTROL/CONNECT 39
.j 255

: 255
> ... done
