#!dimctrl --exec

# ==========================================================================
# Script for taking data when you are tracking wobble position 1

# take a DRS CaLibration and physics Data afterwards
# ==========================================================================

# Move Telescope to Wobble Position 1
>
> --------------------------------------
> data taking for Wobble 1
> starting up...
> --------------------------------------
> OPERATOR:
> make sure the telescope is tracking
> wobble position 1 of the source
> --------------------------------------

# Take a DRS-Calibration before beginning to take physics Data
.x ScriptsForDimCtrl/ServiceScripts/TakeDrsCalibration.dim

> --------------------------------------
> OPERATOR: Measure Sky Brightness
> --------------------------------------

# check feedback state before switching BIAS ON and ramping up to nominal Voltage
.x ScriptsForDimCtrl/ServiceScripts/PrepareBiasForDataTaking.dim

# taking a Data Set (1x Pedestal 1000 Bias On, 1x LPext 1000, 4x5min DataRun)
.x ScriptsForDimCtrl/ServiceScripts/TakeData.dim

> --------------------------------------
> data taking for Wobble 1 finished
> --------------------------------------
