FACT
|<H4>General help about SmartFACT++</h4>||help-main
||
|System status||help-fact-status
|Drive||help-fact-drive
|Relative camera temperature||help-fact-temp
|Humidity / Wind||help-fact-weather
|Trigger rate||help-fact-rate
|G-APD (med/max)||help-fact-bias
|<h4>Event display</h4>
The camera display shows on the last events sent by the fadctrl. For
network traffic reasons only one value, <I>i.e.</i> the maximum
of all four or five pixels, is displayed per bias channel
and the time marker channels are ignored. The extracted value corresponds
to the maximum entry found in the region-of-interest.
|
