#!dimctrl --exec

# ==========================================================================
# changing tracking to "Mrk 421" Wobble 2
# ==========================================================================

>
> moving telescope to wobble position 2
> ...waiting for DRIVE_CONTROL
>    to be in state 6: Armed

DRIVE_CONTROL/STOP
.s DRIVE_CONTROL 6
> ...DRIVE: ARMED
.w 5000

DRIVE_CONTROL/TRACK_SOURCE 0.6 -90 "Mrk 421"
>...sent tracking command for Mrk 421 Wobble 2
> COMMAND: DRIVE_CONTROL/TRACK_SOURCE 0.6 -90 "Mrk 421"
