!Turn voltage off|off
control-irq|This sends the interrupt 'off'. It is supposed to
ramp down the camera voltage, switch off the trigger and close open files.
No other action is taken. The Main script is stopped.|
