*Track Position|doTrackPosition
control-drive|To move the telescope of the given sky coordinates and start 
tracking  press the '&gt;' button at the bottom
of the screen.|
|input=Right ascension [h]/ra/|
|input=Declination [deg]/dec/|
||
|Stop telescope||dodrivestop
