/////////////////////////////////////////////////////////
// Data card template for optimizeCuts executable      //
//                                                     //
// *** Compulsory cards are:                           //
// ONFILES, OFFFILES, OUTFILE                          //
//                                                     //
// the rest are optional                               //
// *** Do NEVER add a datacard with no value after it  //
/////////////////////////////////////////////////////////

// Maximun number of on and off events to be processed)
NEVENTS 9999999

// On data acceptance rate (e.g 4 for taking 1/4 of whole data sample)
ONRATE 3

// Input file name pattern (On data)
ONFILES  /mnt/users/jrico/magic/mars/Mars_Standard02/mtemp/mifae/hillas/mrk20040215OnRotateNoCalB.root

// Input file name pattern (Off data)
OFFFILES  /mnt/users/jrico/magic/mars/Mars_Standard02/mtemp/mifae/hillas/mrk20040215OffRotateA-C.root

// output file name
OUTFILE  ./prueba.out


// Preliminary distance lower and upper cuts (in deg)
DISTCUTS 0.3 1.2

// Size initial, final and number of steps 
// it will take logarithmic constant intervals
// positive number of steps means lower cut (integral)
// negative number of steps means lower and upper cuts (diferential)
SIZECUTS  500 10000 3

// Length initial, final and step values (in deg)
LENGTHCUTS 0.15 0.35 0.1 

// Width initial, final and step values (in deg)
WIDTHCUTS 0.05 0.15 0.1 



