#!/bin/sh
#
# ========================================================================
#
# *
# * This file is part of MARS, the MAGIC Analysis and Reconstruction
# * Software. It is distributed to you in the hope that it can be a useful
# * and timesaving tool in analysing Data of imaging Cerenkov telescopes.
# * It is distributed WITHOUT ANY WARRANTY.
# *
# * Permission to use, copy, modify and distribute this software and its
# * documentation for any purpose is hereby granted without fee,
# * provided that the above copyright notice appear in all copies and
# * that both that copyright notice and this permission notice appear
# * in supporting documentation. It is provided "as is" without express
# * or implied warranty.
# *
#
#
#   Author(s): Daniela Dorner  08/2004 <mailto:dorner@astro.uni-wuerzburg.de>
#
#   Copyright: MAGIC Software Development, 2000-2007
#
#
# ========================================================================
#
# This script launches the filling of the results from the calibration for 
# all sequences of which the results are not yet in the database.
#
# After checking if the script is already running the todolist is written.
# Then for each sequence in the todo list the calibration results are 
# filled into the table Calibration in the database using the macros 
# fillcalib.C and fillsignal.C 
# If this was successful, the status is inserted into the database using 
# the function setstatus.
#

source `dirname $0`/sourcefile
printprocesslog "INFO starting $0"
program=fillcallisto
column=fFillCallisto

set -C

scriptlog=$runlogpath/$program-$datetime.log
date >> $scriptlog 2>&1

# check if the script is already running
lockfile=$lockpath/lock-$program.txt
checklock  >> $scriptlog 2>&1

# get todo file
gettodo  >> $scriptlog 2>&1

cd $mars

# fill information into the database for all sequences in the todo file
for (( s=0 ; s < $num ; s++ ))
do
   sequence=${primaries[$s+$s]}
   telnum=${primaries[$s+$s+1]}
   printprocesslog "INFO starting $program for sequence $sequence"
   no=`printf %08d $sequence | cut -c 0-4`
   no2=`printf %08d $sequence`
   path="$datapath/callisto/$no/$no2"
   signalfile=$path/signal$no2.root
   calibfile=$path/calib$no2.root
   fillcallistologpath=$logpath/$program/$no
   makedir $fillcallistologpath >> $scriptlog 2>&1
   fillcaliblog=$fillcallistologpath/fillcalib-$sequence.log
   fillsignallog=$fillcallistologpath/fillsignal-$sequence.log

   echo "run $program for sequence $sequence" >> $scriptlog 2>&1
   setstatus "start" >> $scriptlog 2>&1
   echo "run fillcalib..." >> $scriptlog 2>&1
   printprocesslog "INFO starting fillcalib for sequence $sequence"

   check1=`root -q -b $macrospath/fillcalib.C+\("\"$calibfile\""\,kFALSE\) | tee $fillcaliblog | intgrep`

   case $check1 in
      1)   echo " check1=$check1 -> everything ok -> run fillsignal " >> $scriptlog 2>&1 
           printprocesslog "INFO done fillcalib successfully for sequence $sequence"
           ;;
      0)   echo " check1=$check1 -> no connection to db -> continue..." >> $scriptlog 2>&1 
           printprocesslog "WARN connection to DB failed"
           check="no"
           setstatus "stop" >> $scriptlog 2>&1
           continue ;;
      *)   echo " check1=$check1 -> ERROR -> step has to be repeated" >> $scriptlog 2>&1
           printprocesslog "ERROR fillcalib failed for sequence $sequence"
           com=$Ffillcalib
           check=$check1
           setstatus "stop" >> $scriptlog 2>&1
           continue ;;
   esac

   printprocesslog "INFO starting fillsignal for sequence $sequence"
   check2=`root -q -b $macrospath/fillsignal.C+\("\"$signalfile\""\,kFALSE\) | tee $fillsignallog | intgrep`
   case $check2 in
      1)   echo " check2=$check2 -> everything ok " >> $scriptlog 2>&1 
           printprocesslog "INFO done fillsignal successfully for sequence $sequence"
           ;;
      0)   echo " check2=$check2 -> no connection to db -> continue..." >> $scriptlog 2>&1 
           printprocesslog "WARN connection to DB failed"
           check="no"
           ;;
      *)   echo " check2=$check2 -> ERROR -> step has to be repeated" >> $scriptlog 2>&1
           printprocesslog "ERROR fillsignal failed for sequence $sequence"
           com=$Ffillsignal
           check=$check2
           ;;
   esac
   
   setstatus "stop" >> $scriptlog 2>&1
done

finish >> $scriptlog 2>&1

