camera 0.5
input_file  /hdb1/users/production/RefData/Proton_20_1_400to409.rfl
#
# Reflector format file that gives the NSB from the stars
starfield_file    /home/magic/RawData/CrabNebula.rfl
#
# Center of the FOV for stars light, right information should
# be here since it is no checked in the Camera program (RA and DEC)
starfield_center  5 34 32 22 00 55
#
# Output file with a brief summary about trigger
data_file test.dat
#
# Root file with the output information
root_file test.root
#
# Information about the telescope
ct_file ../Data/magic.def
#
# Directory to look for the NSB database (it should finish with /)
nsb_directory /tmp/Starlight/
#
# Diskriminator and response properties (gate_lentgh, minimum overlaping time,
# amplitude and fwhm) needed for the trigger studies
trigger_prop 6.0 0.25 1.0 2.0
#
# Trig electronic noise (the width of the gaussian noise is that times
# the amplitude of the single phe response for the trigger)
trig_noise 0.3
#
# Fadc properties (amplitude and fwhm) needed for the fadc simulation
fadc_prop 4.0 5.0
#
# Fadc electronic noise (width of the gaussian on top of FADC signal)
fadc_noise 2.0
#
# Trigger loop mode (theshold, multiplicity and topology)
#trigger_loop 4.0 5.0 0.45 2 4 1 1
#
# Single trigger mode (theshold, multiplicity and topology)
trigger_single 4 4 2
#
# Pixels with special trigger threshold (one line for each pixel)
#pixel_thres 37 7.0
#
# Write also images that do not trigger
write_all_events
#
# Do not write Mc information
#nowrite_McEvt
#
# Do not write Raw Evt information
#nowrite_RawEvt
#
# Write Mc trigger information
write_McTrig
#
# Write Mc fadc information
write_McFadc
#
# Analised pixels
ana_pixels 577
#
# Switch off the Electronic Noise
#elec_noise_off
#
# Switch on NSB
nsb_on
#
# Switch off NSB
#nsb_off
# Number of photons from the diffuse NSB and
# minmum number of phe from shower required to simulate NSB
nsb_mean 0.09 1
#
# Show signal of diskriminator on the screen
#trigger_scan
#
# Show signal of FADC on the screen
#fadc_scan
#
# Select Energy of particles
#select_energy 0 10000000000
#
# Skip showers (interactive)
#skip
#
#Data from STDIN
#data_from_stdin
#
# Seeds for random numbers
seeds 69184 10406
#
# Axis of the telescope while running the reflector simualtion
# 200 400 means that the telescope axis is always paralel to the
# shower axis
telescope_axis 20 90
#
# Distance from source position to camera center (Theta, phi)
source_offset 0.0 0.0
#
# Version of the Corsika, the actual version*1000
corsika_vers 5200
#
# End of steercards
end_file


