Sensor temperatures
|
The displayed values are derived from the 28 working temperature
sensors. The displayed graphics is trigger patch wise  linearly
interpolated or extrapolated. The color scale has its center always
at the average of the 160 calculated temperature values and a range
of +/- 1.5 &deg;C is displayed|
