

**Shutter emergency procedure in case of a general power failure**

Once the telescope has been brought in parking position:

1. Unlock the bolts with a size 4 “hex key” (aka “Allen key” or wrench): 
2. Lock the lids using the small safety springs at the bottom and top of the lid rig;



1. In case of long-lasting power cuts. Place the unbolt stokes of the motors in a safe position and fix them with cable binders.