\section{Results}

\newcommand{\no}{\textcolor{red}{\bf NO\xspace}}
\newcommand{\nt}{\textcolor[rgb]{0.9,0.75,0.}{\scriptsize NOT\xspace}}
\newcommand{\test}{\textcolor[rgb]{0.9,0.75,0.}{\scriptsize TESTED\xspace}}
\newcommand{\ok}{\textcolor[rgb]{0.,.7,0.}{OK\xspace}}
\newcommand{\best}{\textcolor[rgb]{0.,.4,0.}{\bf BEST\xspace}}

\begin{table}[htp]
\centering
\small{
\begin{tabular}{|c|c|c|c|c|c|c|c|c|c|c|}
\hline
\hline
\multicolumn{11}{|c|}{\large Tested Characteristics} \rule{0mm}{6mm} \rule[-2mm]{0mm}{6mm} \hspace{-3mm}\\
\hline
\hline
Nr. & Name         &  Res.  & Bias &    Stab. & Stab.  &  Stab. & Res. & Stab.  & Lin. & Speed \\
    &              &   $\widehat{S}$     & $\widehat{S}$  &  $\widehat{S}$  &  pulse & low- & $\widehat{T}$ & $\widehat{T}$ &  $\widehat{S}$  & \\
    &              &      &     &   &  shape & gain & & &  &  \\
\hline                                                     
\hline                                                     
1   & Fix Win. (4,4)   & \no & -- & \ok & \no & \no & n/a & n/a & \no & \best \\   
2   & Fix Win. (4,6)   & \ok & -- & \ok & \no & \no & n/a & n/a & \no   & \best \\   
3   & Fix Win. (6.6)   & \ok & -- & \ok & \ok & \no & n/a & n/a & \ok   & \ok \\   
4   & Fix Win. (8,8)   & \no & -- & \ok & \ok & \ok & n/a & n/a & \best & \ok \\   
5   & Fix W. (14,10)   & \no & -- & \no & \ok & \ok & n/a & n/a & \best & \ok \\   
\hline                                 
6   & FW. Spl. (4,4) & \no  & -- & \ok & \no & \no & n/a  &  n/a & \no & \ok \\   
7   & FW. Spl. (4,6) & \ok  & -- & \ok & \no & \no & n/a  &  n/a & \no & \ok \\   
8   & FW. Spl. (6.6) & \ok  & -- & \ok & \ok & \no & n/a  &  n/a & \no & \ok \\   
9   & FW. Spl. (8,8) & \no  & -- & \ok & \ok & \ok & n/a  &  n/a & \ok & \ok \\   
10  & FW. Spl (14,10) & \no  & -- & \no & \ok & \ok & n/a  &  n/a & \ok & \ok \\   
\hline                                
11  & FW. Pk S. (2,2)& \no  & -- & \no & \no & \no & n/a  &  n/a & \no & \ok \\   
12  & FW. Pk S. (4,4)& \no  & -- & \ok & \no & \no & n/a  &  n/a & \no & \ok \\   
13  & FW. Pk S. (4.6)& \ok  & -- & \ok & \no & \no & n/a  &  n/a & \no & \ok \\   
14  & FW. Pk S. (6,6)& \ok  & -- & \ok & \ok & \no & n/a  &  n/a & \no & \ok \\   
15  & FW. Pk S. (8,8)& \no  & -- & \ok & \ok & \ok & n/a  &  n/a & \ok & \ok \\   
16  & FW Pk S (14,10)& \no  & -- & \no & \ok & \ok & n/a  &  n/a & \ok & \ok \\   
\hline                                
17  & Slid. W. (2,2)       & \ok & \ok & \ok & \no & \no & \no & \no & \no & \ok \\   
18  & Slid. W. (4,4)       & \ok & \ok & \ok & \ok & \ok & \no & \no & \no & \ok \\   
19  & Slid. W. (4.6)       & \ok & \ok & \ok & \ok & \ok & \ok & \no & \ok & \ok \\   
20  & Slid. W. (6,6)       & \no & \ok & \ok & \ok & \ok & \no & \ok & \ok & \ok \\   
21  & Slid. W. (8,8)       & \no & \ok & \ok & \ok & \ok & \ok & \ok & \ok & \ok \\   
22  & Slid. W. (14,10)       & \no & \ok & \ok & \ok & \ok & \no & \ok & \ok & \ok \\   
\hline                                
23  & Spline Ampl.           & \ok & \no & \no & \nt   & \ok & \ok   & \no & \no & \ok \\
    &                        &     &     &     & \test &     &       &     &     &     \\
24  & Splne Int. (1,1.5)     & \ok & \ok & \ok & \nt   & \ok & \best & \ok & \no & \ok \\
    &                        &     &     &     & \test &     &       &     &     &     \\
25  & Spline Int. (2,3)      & \ok &\ok  & \best&\nt   & \ok & \best & \ok & \ok & \no \\
    &                        &     &     &     & \test &     &       &     &     &     \\
26  & Spline Int. (4,6)      & \ok &\ok  & \ok & \ok & \ok & \best & \ok & \ok & \no \\
27  & Spline Int. (6,9)      & \no &\best& \ok & \ok & \ok & \best & \ok & \ok & \no \\
\hline                                                                          
28  & Dig. Filt. (6,6)       & \ok   &\ok & \ok & \ok  & \ok & \ok  & \ok & \ok & \ok \\
29  & Dig. Filt. (4,4)       & \best &\ok & \ok & \ok  & \ok & \best& \ok & \ok & \ok \\
\hline
\hline
\end{tabular}
}
\caption{The tested characteristics for every extractor: Bias, Resolution (``Res.''), stability (``Stab.''), linearity (``Lin.'') for both 
charge signal $\widehat{S}$ and time $\widehat{T}$, and speed. \ok\ means that the extractor has passed the 
test, without being among the best. \no\ means that the extractor has severely failed the test and should 
not be taken because of that reason. \best\ means that the extractor(s) have come out as best of the particular test.
}
\label{tab:result}
\end{table}



%%% Local Variables: 
%%% mode: latex
%%% TeX-master: "MAGIC_signal_reco"
%%% End: 
