camera 0.3
# Reflector file that the program reads
input_file /hdb1/users/blanch/Ref_pro/prova.rfl
#
# Reflector format file that gives the NSB from the stars
starfield_file    /hdb1/users/blanch/Starfield/Ref_stf1
#
# Output file with a brief summary about trigger
data_file /hdb1/users/blanch/test.dat
#
# Root file with the output information
root_file /hdb1/users/blanch/Cam_test.root
#
# Information about the telescope
ct_file ../Data/magic.def
#
# Diskriminator and response properties (gate_lentgh, amplitude and fwhm)
# needed for the trigger studies
trigger_prop 3.0 1.0 2.0
#
# Trigger loop mode (theshold, multiplicity and topology)
trigger_loop 0 2 4 4 1 1
#
# Single trigger mode (theshold, multiplicity and topology)
#trigger_single 4 4 1
#
# Write also images that do not trigger
#write_all_images
#
# Analised pixels
ana_pixels 595
#
# Switch on NSB
#nsb_on
#
# Switch off NSB
nsb_off
# Number of photon from the diffuse NSB
nsb_mean 0.09
#
# Show signal of diskriminator on the screen
#trigger_scan
#
# Show signal of FADC on the screen
#fadc_scan
#
# Select Energy of particles
#select_energy 0 10000000000
#
# Skip showers (interactive)
#skip
#
#Data from STDIN
#data_from_stdin
#
# Seeds for random numbers
seeds 69184 10406
#
# End of steercards
end_file
